IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2023-03-10T15:02:41"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Alternate UI 20.2.90.12"
Application: "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)"

People and organizations
  Person "erin.hay" of Organization (no name given)
  Owner history of Person "erin.hay" of Organization (no name given) | application "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)" | change NOCHANGE | created 1678460560 (2023-03-10T15:02:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | type IFCCOVERINGTYPE "AgedCedar" | object type "NBS_TapcoRoofingProducts_RcnstttdSltCrsngFitngs_DaVinciSelectShakeRidgeAndHipCap:AgedCedar" | ROOFING | names: "NBS_TapcoRoofingProducts_RcnstttdSltCrsngFitngs_DaVinciSelectShakeRidgeAndHipCap:AgedCedar:318093" | material: "NBS_TapcoRoofingProducts_AgedCedar" | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "AgedCedar" | ROOFING | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  IFC | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "ROOFING" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_90_93_29:Dry fixing ridges" (IFCTEXT)
    CodePerformance = "To EN 13501-5, BROOF(t4); Hail rating Class 4 UL 2218" (IFCTEXT)
    Color = "Black,Brown" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "A dry-fix ridge and hip cap for all roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Ridges and hips are mechanically fixed, choice of three colours to match the Select Shake tiles, fully tested to BBA standards, including fire rating, wind, driven snow and rain, and water absorption" (IFCTEXT)
    Finish = "Woodgrain" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "info@tapcoslate.com" (IFCTEXT)
    Material = "NBS_TapcoRoofingProducts_AgedCedar" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "DaVinci Select Shake Ridge and Hip Caps" (IFCTEXT)
    Name = "DryFixingRidges_DaVinciSelectShakeRidgeAndHipCaps_AgedCedar_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 465. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 302. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Other" (IFCTEXT)
    Size = "465 x 302 mm" (IFCTEXT)
    SustainabilityPerformance = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_90_93_29:Dry fixing ridges" (IFCTEXT)
    CodePerformance = "To EN 13501-5, BROOF(t4); Hail rating Class 4 UL 2218" (IFCTEXT)
    Color = "Black,Brown" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "A dry-fix ridge and hip cap for all roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Ridges and hips are mechanically fixed, choice of three colours to match the Select Shake tiles, fully tested to BBA standards, including fire rating, wind, driven snow and rain, and water absorption" (IFCTEXT)
    Finish = "Woodgrain" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@tapcoslate.com" (IFCTEXT)
    Material = "NBS_TapcoRoofingProducts_AgedCedar" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "DaVinci Select Shake Ridge and Hip Caps" (IFCTEXT)
    Name = "DryFixingRidges_DaVinciSelectShakeRidgeAndHipCaps_AgedCedar_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 465. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 302. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Other" (IFCTEXT)
    Size = "465 x 302 mm" (IFCTEXT)
    SustainabilityPerformance = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    WarrantyDescription = "40 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_DryFixingRidges_DaVinciSelectShakeRidge&HipCaps_AgedCedar" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSInstanceId = "8821bbdf-7cdb-445a-bb53-3dfe837d31da" (IFCTEXT)
    NBSObjectId = "5f42ca6f-9695-4291-a67d-1041d41023c2" (IFCTEXT)
    NBSVariantId = "e01b2727-56a0-ac81-1c7b-a2fdbdb3b848" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/5f42ca6f-9695-4291-a67d-1041d41023c2/8821bbdf-7cdb-445a-bb53-3dfe837d31da" (IFCTEXT)
    Uniclass2015Code = "Pr_35_90_93_29" (IFCTEXT)
    Uniclass2015Title = "Dry fixing ridges" (IFCTEXT)
    Uniclass2015Version = "Products v1.29" (IFCTEXT)
    Version = "2" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCBUILDING)
    Author (no value)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Colour = "Aged cedar" (IFCTEXT)
    Construction = "Composite blend of virgin polyethylene, UV and thermal stabilizers as well as a highly specialized fire retardant" (IFCTEXT)
    CountryOfMaterialOrigin = "United States" (IFCTEXT)
    CountryOfProductManufacture = "United States" (IFCTEXT)
    Dimensions = "302 x 465 mm" (IFCTEXT)
    FireRating = "To EN 13501-5, BROOF(t4)" (IFCTEXT)
    Form = "Duo-ridge unventilated dry fixing kits" (IFCTEXT)
    Recyclability = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    Thickness = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Weight = "1 kg" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "London", "London", "United Kingdom"