IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2023-03-10T15:10:18"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Alternate UI 20.2.90.12"
Application: "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)"

People and organizations
  Person "erin.hay" of Organization (no name given)
  Owner history of Person "erin.hay" of Organization (no name given) | application "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)" | change NOCHANGE | created 1678458496 (2023-03-10T14:28:16Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 3 elements
          1 x IFCROOF | object type "Basic Roof:NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_AgedCedar" | names: "Basic Roof:NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_AgedCedar:221698" | parts: 1 IFCSLAB | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCROOF | object type "Basic Roof:NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_BlackOak" | names: "Basic Roof:NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_BlackOak:221866" | parts: 1 IFCSLAB | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCROOF | object type "Basic Roof:NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_Autumn" | names: "Basic Roof:NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_Autumn:221922" | parts: 1 IFCSLAB | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  IFC | properties | on 6 objects (3 IFCROOF, 3 IFCSLAB)
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "ROOFING" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_93_72_96:Wood shakes" (IFCTEXT)
    CodePerformance = "To BS EN 13501-5, BROOF(t4); Hail rating Class 4 UL 2218" (IFCTEXT)
    Color = "Brown,Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Dry-fix starter or eaves tile for all roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Constructed of a composite material made of virgin resins, UV and thermal stabilizers as well as a highly-specialized fire retardant" (IFCTEXT)
    Finish = "Woodgrain" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "info@tapcoslate.com" (IFCTEXT)
    Material = "Polyethylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "DaVinci Select Shake Starter Tiles" (IFCTEXT)
    Name = "WoodShakes_DaVinciSelectShakeStarterTiles_AgedCedar_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 305. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "350 x 305 x 6 mm" (IFCTEXT)
    SustainabilityPerformance = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_93_72_96:Wood shakes" (IFCTEXT)
    CodePerformance = "To BS EN 13501-5, BROOF(t4); Hail rating Class 4 UL 2218" (IFCTEXT)
    Color = "Brown,Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Dry-fix starter or eaves tile for all roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Constructed of a composite material made of virgin resins, UV and thermal stabilizers as well as a highly-specialized fire retardant" (IFCTEXT)
    Finish = "Woodgrain" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "info@tapcoslate.com" (IFCTEXT)
    Material = "Polyethylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "DaVinci Select Shake Starter Tiles" (IFCTEXT)
    Name = "WoodShakes_DaVinciSelectShakeStarterTiles_BlackOak_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 305. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "350 x 305 x 6 mm" (IFCTEXT)
    SustainabilityPerformance = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_93_72_96:Wood shakes" (IFCTEXT)
    CodePerformance = "To BS EN 13501-5, BROOF(t4); Hail rating Class 4 UL 2218" (IFCTEXT)
    Color = "Brown,Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Dry-fix starter or eaves tile for all roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Constructed of a composite material made of virgin resins, UV and thermal stabilizers as well as a highly-specialized fire retardant" (IFCTEXT)
    Finish = "Woodgrain" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "info@tapcoslate.com" (IFCTEXT)
    Material = "Polyethylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "DaVinci Select Shake Starter Tiles" (IFCTEXT)
    Name = "WoodShakes_DaVinciSelectShakeStarterTiles_Autumn_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 305. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "350 x 305 x 6 mm" (IFCTEXT)
    SustainabilityPerformance = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)
  BOS_General | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_AgedCedar" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSInstanceId = "61f6853a-3114-4240-aac9-fa11c921ce99" (IFCTEXT)
    NBSObjectId = "f38f8095-25fd-4348-9372-f136dd72a6c2" (IFCTEXT)
    NBSVariantId = "82243149-2f50-4be3-b513-6bf20fe727c7" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/f38f8095-25fd-4348-9372-f136dd72a6c2/61f6853a-3114-4240-aac9-fa11c921ce99" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_96" (IFCTEXT)
    Uniclass2015Title = "Wood shakes" (IFCTEXT)
    Uniclass2015Version = "Products v1.29" (IFCTEXT)
    Version = "2" (IFCTEXT)
  BOS_General | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_BlackOak" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSInstanceId = "61f6853a-3114-4240-aac9-fa11c921ce99" (IFCTEXT)
    NBSObjectId = "f38f8095-25fd-4348-9372-f136dd72a6c2" (IFCTEXT)
    NBSVariantId = "71cf9990-7dc4-48fd-8bd5-b9c2dbf9b1eb" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/f38f8095-25fd-4348-9372-f136dd72a6c2/61f6853a-3114-4240-aac9-fa11c921ce99" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_96" (IFCTEXT)
    Uniclass2015Title = "Wood shakes" (IFCTEXT)
    Uniclass2015Version = "Products v1.29" (IFCTEXT)
    Version = "2" (IFCTEXT)
  BOS_General | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_WoodShakes_DaVinciSelectShakeStarterTiles_Autumn" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSInstanceId = "61f6853a-3114-4240-aac9-fa11c921ce99" (IFCTEXT)
    NBSObjectId = "f38f8095-25fd-4348-9372-f136dd72a6c2" (IFCTEXT)
    NBSVariantId = "f7370773-b0e4-4f7d-89a0-df962885bada" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/f38f8095-25fd-4348-9372-f136dd72a6c2/61f6853a-3114-4240-aac9-fa11c921ce99" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_96" (IFCTEXT)
    Uniclass2015Title = "Wood shakes" (IFCTEXT)
    Uniclass2015Version = "Products v1.29" (IFCTEXT)
    Version = "2" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCBUILDING)
    Author (no value)
  NBS_Data | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Colour = "Aged cedar" (IFCTEXT)
    CountryOfMaterialOrigin = "United States" (IFCTEXT)
    CountryOfProductManufacture = "United States" (IFCTEXT)
    Form = "Composite blend of virgin polyethylene, UV and thermal stabilizers and specialized fire retardant" (IFCTEXT)
    LengthMinimum = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Recyclability = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    Thickness = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    TreatmentFlameRetardance = "To EN 13501-5, BROOF(t4)" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
    Width = 305. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Colour = "Black oak" (IFCTEXT)
    CountryOfMaterialOrigin = "United States" (IFCTEXT)
    CountryOfProductManufacture = "United States" (IFCTEXT)
    Form = "Composite blend of virgin polyethylene, UV and thermal stabilizers and specialized fire retardant" (IFCTEXT)
    LengthMinimum = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Recyclability = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    Thickness = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    TreatmentFlameRetardance = "To EN 13501-5, BROOF(t4)" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
    Width = 305. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Colour = "Autumn" (IFCTEXT)
    CountryOfMaterialOrigin = "United States" (IFCTEXT)
    CountryOfProductManufacture = "United States" (IFCTEXT)
    Form = "Composite blend of virgin polyethylene, UV and thermal stabilizers and specialized fire retardant" (IFCTEXT)
    LengthMinimum = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Recyclability = "Manufactured from recyclable virgin polyethylene" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    Thickness = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    TreatmentFlameRetardance = "To EN 13501-5, BROOF(t4)" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
    Width = 305. (IFCLENGTHMEASURE) [MILLI METRE]

Other addresses and roles
  2 x postal address: "Enter address here", "Westminster", "London", "UK"