IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2021-07-21T18:41:03"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210416_1515(x64) - Exporter 19.2.30.41 - Alternate UI 19.2.30.41"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "elisabeth.kitumaini" of Organization (no name given)
  Owner history of Person "elisabeth.kitumaini" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1626889263 (2021-07-21T17:41:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | object type "NBS_TapcoRoofingProducts_DryFxngHips_HipMaster:HipMaster" | ROOFING | names: "NBS_TapcoRoofingProducts_DryFxngHips_HipMaster:HipMaster:4688" | material: "NBS_TapcoRoofingProducts_Polypropylene_Black" | property sets: BOS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie

Property sets
  BOS_General | properties | on 1 object (1 IFCCOVERING)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_DryFixingHips_HipMaster" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/r5omdyc1" (IFCTEXT)
    NBSDescription = "Dry fixing hips" (IFCTEXT)
    NBSReference = "45-80-90/374" (IFCTEXT)
    ProductInformation = "HipMaster Roofing Hip Ventilation | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_35_90_93_28" (IFCTEXT)
    Uniclass2015Title = "Dry fixing hips" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    Accessories = "n/a" (IFCTEXT)
    Applications = "Suitable for use with the TapcoSlate Classic Ridge/ Hip system, for roof pitches 14 to 45 degrees" (IFCTEXT)
    Form = "n/a" (IFCTEXT)
    PitchRange = "14° - 45°" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  IFC | properties | on 1 object (1 IFCCOVERING)
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "ROOFING" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_90_93_28:Dry fixing hips" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "A dry-fix hip ventilation system that fits underneath the TapcoSlate Classic Ridge/ Hip system" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "50+ years" (IFCTEXT)
    Features = "Enhanced roof ventilation at the hip, patented triple-baffle system engineered to keep blowing rain and snow from getting in, internal filter blocks out insects, leaves and other debris, the low-profile design is unobtrusive, nailing supports and structural ribs make the Hip Master crushproof, to withstand falling tree branches and hammer blows, and it resists cracking, self-aligning, interlocking ends make it easy to install correctly, built-in end caps adjust to the roof pitch while the ship-lap design allows for expansion and contraction as temperatures change, can be joined with Ridge Master Plus ridge ventilation, 10 000 mm²/m ventilation provision to comply with building regulations for both warm and cold roofs" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene (PP) and Rubber" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "HipMaster" (IFCTEXT)
    Name = "DryFixingHips_HipMaster_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 35.0000000532 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1219.00000185288 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 270.0000004104 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "1219 x 270 x 35 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 1" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)