IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2021-07-06T12:44:00"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1625571840 (2021-07-06T11:44:00Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1625571840 (2021-07-06T11:44:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" | ROOF | names: "NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" 2.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" 2.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_10_94:Vapour permeable sheets" (IFCTEXT)
    CodePerformance = "BS 5250, BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Medium-weight, vapour permeable roofing underlay" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Easy to cut and lightweight to handle, highly vapour permeable, but entirely watertight, UV stable and heat resistant, helps to avoid condensation risk in the roof space, for use in zones 1–5 at 250 mm batten gauge in regard to wind uplift, can be used as temporary roof covering" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Non-woven spunbonded polypropylene" (IFCTEXT)
    ModelNumber = "VP300" (IFCTEXT)
    ModelReference = "VP300_Membrane" (IFCTEXT)
    Name = "VapourPermeableSheets_VP300_Membrane_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 50000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Roll" (IFCTEXT)
    Size = "50000 x 1000 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "Embossed" (IFCTEXT)
    FireRating = "Class F" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable and recommended for all Tapco Roofing products, suitable for use in cold or warm pitched roof constructions" (IFCTEXT)
    ClassMinimum = "W1" (IFCTEXT)
    Form = "Non-woven Spun-bond" (IFCTEXT)
    PerformanceRequirement = "Water vapour resistance to BS EN ISO 12572; 0.17 MNs/g and 0.022 Sd Wind Uplift Resistance to BS5534 Zones 1-3 (345mm batten gauge)" (IFCTEXT)
    ReflectiveFace = "n/a" (IFCTEXT)
    StandLength = "50,000 mm" (IFCTEXT)
    Standard = "BS 5250, BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    ThicknessMinimum = "0.6mm" (IFCTEXT)
    ThirdPartyCertification = "BS 5250, BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    WeightMinimum = "6.55 kg" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_VapourPermeableSheets_VP300_Membrane" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/hay0db5n" (IFCTEXT)
    NBSDescription = "Vapour permeable sheets" (IFCTEXT)
    NBSReference = "45-65-50/323" (IFCTEXT)
    ProductInformation = "Protect VP300 Underlay | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_10_94" (IFCTEXT)
    Uniclass2015Title = "Vapour permeable sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)