IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2021-07-06T12:44:00"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1625571840 (2021-07-06T11:44:00Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1625571840 (2021-07-06T11:44:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 3 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" | ROOF | names: "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" 2.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" | ROOF | names: "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" 2.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" | ROOF | names: "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" 2.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" 2.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" 2.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" ("NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" 2.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General

Property sets
  COBie | properties | on 3 objects (3 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_10_94:Vapour permeable sheets" (IFCTEXT)
    CodePerformance = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Light-weight roofing underlay" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Easy to cut, clean and light to handle, proven time saving over traditional felts, for use in zones 1–4 at 345 mm batten gauge, completely waterproof, excellent nail tear and tensile strength" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Non-woven spunbonded polypropylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Wunderlay_15000mm_Membrane" (IFCTEXT)
    Name = "VapourPermeableSheets_Wunderlay_15000mm_Membrane_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 15000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Roll" (IFCTEXT)
    Size = "15000 x 1000 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_10_94:Vapour permeable sheets" (IFCTEXT)
    CodePerformance = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Light-weight roofing underlay" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Easy to cut, clean and light to handle, proven time saving over traditional felts, for use in zones 1–4 at 345 mm batten gauge, completely waterproof, excellent nail tear and tensile strength" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Non-woven spunbonded polypropylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Wunderlay_30000mm_Membrane" (IFCTEXT)
    Name = "VapourPermeableSheets_Wunderlay_30000mm_Membrane_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 30000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Roll" (IFCTEXT)
    Size = "30000 x 1000 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_10_94:Vapour permeable sheets" (IFCTEXT)
    CodePerformance = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Light-weight roofing underlay" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Easy to cut, clean and light to handle, proven time saving over traditional felts, for use in zones 1–4 at 345 mm batten gauge, completely waterproof, excellent nail tear and tensile strength" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Non-woven spunbonded polypropylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Wunderlay_45000mm_Membrane" (IFCTEXT)
    Name = "VapourPermeableSheets_Wunderlay_45000mm_Membrane_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 45000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Roll" (IFCTEXT)
    Size = "45000 x 1500 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 3 type objects
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 3 type objects
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "Class F" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable and recommended for all Tapco Roofing products, can be used as temporary roof covering" (IFCTEXT)
    ClassMinimum = "W1" (IFCTEXT)
    Form = "Non-woven Spun-bond" (IFCTEXT)
    PerformanceRequirement = "Impermeable, Wind Uplift Resistance to BS5534 Zones 1-4 (345mm batten gauge)" (IFCTEXT)
    ReflectiveFace = "n/a" (IFCTEXT)
    StandLength = "15,000 mm" (IFCTEXT)
    Standard = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    ThicknessMinimum = "0.49mm" (IFCTEXT)
    ThirdPartyCertification = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    WeightMinimum = "5.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable and recommended for all Tapco Roofing products, can be used as temporary roof covering" (IFCTEXT)
    ClassMinimum = "W1" (IFCTEXT)
    Form = "Non-woven Spun-bond" (IFCTEXT)
    PerformanceRequirement = "Impermeable, Wind Uplift Resistance to BS5534 Zones 1-4 (345mm batten gauge)" (IFCTEXT)
    ReflectiveFace = "n/a" (IFCTEXT)
    StandLength = "30,000 mm" (IFCTEXT)
    Standard = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    ThicknessMinimum = "0.49mm" (IFCTEXT)
    ThirdPartyCertification = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    WeightMinimum = "5.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable and recommended for all Tapco Roofing products, can be used as temporary roof covering" (IFCTEXT)
    ClassMinimum = "W1" (IFCTEXT)
    Form = "Non-woven Spun-bond" (IFCTEXT)
    PerformanceRequirement = "Impermeable, Wind Uplift Resistance to BS5534 Zones 1-4 (345mm batten gauge)" (IFCTEXT)
    ReflectiveFace = "n/a" (IFCTEXT)
    StandLength = "45,000 mm" (IFCTEXT)
    Standard = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    ThicknessMinimum = "0.49mm" (IFCTEXT)
    ThirdPartyCertification = "BM TRADA Q-Mark Certification/ CE Marked" (IFCTEXT)
    WeightMinimum = "5.7 kg" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_15000mm_Membrane" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/51oac0tn" (IFCTEXT)
    NBSDescription = "Vapour permeable sheets" (IFCTEXT)
    NBSReference = "45-65-50/323" (IFCTEXT)
    ProductInformation = "Protect Wunderlay | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_10_94" (IFCTEXT)
    Uniclass2015Title = "Vapour permeable sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_30000mm_Membrane" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/51oac0tn" (IFCTEXT)
    NBSDescription = "Vapour permeable sheets" (IFCTEXT)
    NBSReference = "45-65-50/323" (IFCTEXT)
    ProductInformation = "Protect Wunderlay | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_10_94" (IFCTEXT)
    Uniclass2015Title = "Vapour permeable sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_VapourPermeableSheets_Wunderlay_45000mm_Membrane" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/51oac0tn" (IFCTEXT)
    NBSDescription = "Vapour permeable sheets" (IFCTEXT)
    NBSReference = "45-65-50/323" (IFCTEXT)
    ProductInformation = "Protect Wunderlay | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_10_94" (IFCTEXT)
    Uniclass2015Title = "Vapour permeable sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)