IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2021-07-06T12:44:00"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1625571840 (2021-07-06T11:44:00Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1625571840 (2021-07-06T11:44:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" 2.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" 2.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_90_93_72:Reconstituted slate roof slope ventilation fittings" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Eaves rafter roll ventilator for warm roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Provides ventilation opening of 25 000 mm²/m, quick and easy to install, lightweight and durable, compatible with all roof tile clips and eaves fillers, does not effect slating/ tiling process, gutter bracket spacers available to ensure correct gutter position and unrestricted airflow, kit comprises 6 lengths of 25mm over fascia vent and 10 eaves skirts" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Injection moulded polypropylene" (IFCTEXT)
    ModelNumber = "TEVK25" (IFCTEXT)
    ModelReference = "TEVK25_RafterRollVentilator" (IFCTEXT)
    Name = "ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 6000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  NBS_Data | properties | on 1 type object
    Applications = "For warm roof installations, to be used in conjunction with all Tapco Roofing products, especially suitable for Tapco Slate Classic tiles" (IFCTEXT)
    Colour = "Black" (IFCTEXT)
    Form = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_TEVK25_RafterRollVentilator" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/rofwlcdd" (IFCTEXT)
    NBSDescription = "Reconstituted slates roof slope ventilation fittings" (IFCTEXT)
    NBSReference = "45-80-90/392" (IFCTEXT)
    ProductInformation = "Tapco Eaves Ventilation Kits | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_35_90_93_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted slate roof slope ventilation fittings" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)