IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2021-07-27T13:23:14"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210416_1515(x64) - Exporter 19.2.30.41 - Alternate UI 19.2.30.41"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "elisabeth.kitumaini" of Organization (no name given)
  Owner history of Person "elisabeth.kitumaini" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1627388593 (2021-07-27T12:23:13Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | object type "NBS_TapcoRoofingProducts_RcnstttdSltCrsngFitngs_TapcoSlate_ClassicRidgeToHipJunction:TapcoSlate_ClassicRidgeToHipJunction_706Plum_14To17DegPitch" | ROOFING | names: "NBS_TapcoRoofingProducts_RcnstttdSltCrsngFitngs_TapcoSlate_ClassicRidgeToHipJunction:TapcoSlate_ClassicRidgeToHipJunction_706Plum_14To17DegPitch:3527" | material: "NBS_TapcoRoofingProducts_Slate_706Plum" | property sets: BOS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie

Property sets
  BOS_General | properties | on 1 object (1 IFCCOVERING)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesCoursingFittings_TapcoSlate_ClassicRidgeToHipJunction_706Plum_14To17DegPitch" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/2omsavt2" (IFCTEXT)
    NBSDescription = "Reconstituted slates coursing fittings" (IFCTEXT)
    NBSReference = "45-80-90/388" (IFCTEXT)
    ProductInformation = "https://www.tapcoroofingproducts.com/product/tapcoslate-classic-angled-ridge-hip-cap/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_73" (IFCTEXT)
    Uniclass2015Title = "Reconstituted slate coursing fittings" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    Applications = "Suitable for Tapco Slate Classic and Tapco Slate Classic Ridge and Hip Caps, it is especially valuable for the 3-way junction on an Edwardian conservatory roof" (IFCTEXT)
    Colour = "Plum" (IFCTEXT)
    Fittings = "n/a" (IFCTEXT)
    PitchRange = "14° - 17°" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "BS476 Part 3, Boarded Roof SAA, Battened Roof SAC" (IFCTEXT)
    FlammabilityRating = "BS476 Part 3, Boarded Roof SAA, Battened Roof SAC" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  IFC | properties | on 1 object (1 IFCCOVERING)
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "ROOFING" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Generic Models" (IFCTEXT)
    CodePerformance = "Fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Plum" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "A dry-fix ridge to hip junction cap for all roofs where the ridge meets the hip" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg per square metre, easy to install with pre-marked nailing guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, mechanically fixed" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Virgin limestone, polypropylene" (IFCTEXT)
    ModelNumber = "706" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicRidgeToHipJunction_706Plum_14To17DegPitch" (IFCTEXT)
    Name = "ReconstitutedSlatesCoursingFittings_TapcoSlate_ClassicRidgeToHipJunction_706Plum_14To17DegPitch_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 45.0000000684 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445.0000006764 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 300.000000456 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "45 x 445 x 300 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 1" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)