IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2021-07-06T12:43:59"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1625571840 (2021-07-06T11:44:00Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1625571840 (2021-07-06T11:44:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 8 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" 5.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" 5.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" 5.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General

Property sets
  COBie | properties | on 8 objects (8 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Stone black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "801" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_801StoneBlack" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Pewter grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "804" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_804PewterGrey" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Red rock" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "809" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_809RedRock" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Olive green" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "814" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_814OliveGreen" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Plum" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "706" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_706Plum" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Brick red" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "709" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_709BrickRed" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_93_72_72:Reconstituted interlocking slates" (IFCTEXT)
    CodePerformance = "BS476 Part 3, fully tested to BBA, ETA and CE standards" (IFCTEXT)
    Color = "Chestnut brown" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Authentically shaped classic roof tiles with textured surfaces and riven edges moulded from authentic slates" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "80+ years" (IFCTEXT)
    Features = "Lightweight – as low as 12 kg/m², easy to install with pre-marked nailing and exposure guides and spacers, easily cut with a fine-toothed saw or sharp utility blade, built-in camber for tighter fit when fixed in situ, no sorting, clipping or drilling prior to roof loading, packaged in bundles of twenty-five for easy handling, fittings (ridges and hips) are mechanically fixed, local Authority Building Control (LABC) & Local Authority Building Standards Scotland (LABSS) Registered Details product, BRE testing for wind-driven rain found TapoSlate Classic to perform more strongly than all equivalent materials tested and at a lower pitch" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polypropylene, limestone" (IFCTEXT)
    ModelNumber = "712" (IFCTEXT)
    ModelReference = "TapcoSlate_ClassicTile_712ChestnutBrown" (IFCTEXT)
    Name = "ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 445. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 292. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "5 x 445 x 292 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie: 1 more content on 0 objects not shown
  xbim_MaterialFunctionAssignment | properties | on 8 type objects
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 8 type objects
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "BS476 Part 3, Boarded Roof SAA, Battened Roof SAC" (IFCTEXT)
    FlammabilityRating = "BS476 Part 3, Boarded Roof SAA, Battened Roof SAC" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Stone black" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Pewter grey" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Red rock" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Olive green" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Plum" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Brick red" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Chestnut brown" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Suitable for conservatories, modern houses or listed buildings" (IFCTEXT)
    Colour = "Coachman mix" (IFCTEXT)
    CoverageHip = "5.5 to 6.5 per linear metre (depending on gauge)" (IFCTEXT)
    CoverageRidgeGap = "5.5 per linear metre" (IFCTEXT)
    CoverageSlate = "22 slates/sq. metre at 14° to 25°, 20 slates/sq. metre at 25° to 27.5°, 19 slates/sq. metre at 27.5° to 30°, 18 slates/sq. metre above 30°" (IFCTEXT)
    Cutting = "Fine-toothed handsaw, jigsaw, circular saw, or sharp utility blade" (IFCTEXT)
    Fixing = "Large-headed galvanised 1.2” (30mm) by 0.1” (2.5mm) steel nails (using hammer or nail-gun), aluminium or copper nails may also be used, but driving them through the slate may cause bending, longer 3” (76mm) nail required for fixing ridges and hips" (IFCTEXT)
    Gauge = "6” at 14° to 25°, 6.5” at 25° to 27.5°, 7” at 27.5° to 30°, 7.5” above 30°" (IFCTEXT)
    PitchRange = "14° - 90°" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Weight = "0.7 kg" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_801StoneBlack" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_804PewterGrey" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_809RedRock" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_814OliveGreen" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_706Plum" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_709BrickRed" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_712ChestnutBrown" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesInterlocking_TapcoSlate_ClassicTile_790CoachmanMix" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/t1jt0vvl" (IFCTEXT)
    NBSDescription = "Reconstituted slates interlocking" (IFCTEXT)
    NBSReference = "45-80-90/390" (IFCTEXT)
    ProductInformation = "TapcoSlate Classic Roof Tile | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_93_72_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted interlocking slates" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)