IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2021-07-06T12:44:00"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1625571841 (2021-07-06T11:44:01Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1625571841 (2021-07-06T11:44:01Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" | ROOF | names: "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" 2.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" | ROOF | 1 occurrence | material: layers "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" ("NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" 2.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_90_93_72:Reconstituted slate roof slope ventilation fittings" (IFCTEXT)
    CodePerformance = "BS 5250" (IFCTEXT)
    Color = "Vacuum-formed Black PVC" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Rafter roll ventilator installed with fascia ventilators or soffit ventilators to provide a continuous ventilation path from the roof void to the outside without impairing the weatherproof function of the structure" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Does not affect the slating/tiling process, unique cross strengthening ribs on rafter trays prevent the underlay from sagging and blocking the airflow, reduce the risk of cold bridging by enabling insulation to be laid right into the eaves, lightweight and durable, quick and easy to install, with no special tools required, suits standard rafter spacing, independent of soffit and fascia ventilators, enabling use with any depth of soffit" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Polyvinyl chloride (PVC)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "450mmRafterRollVentilator" (IFCTEXT)
    Name = "ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 6000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "6000 x 450 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  NBS_Data | properties | on 1 type object
    AirFlow = "25,000mm²/m" (IFCTEXT)
    Applications = "Suitable and recommended for all Tapco Roofing products, designed to ensure a clear air path between roof underlay and insulation at all types of eaves" (IFCTEXT)
    Colour = "Vacuum-formed Black PVC" (IFCTEXT)
    Coverage = "12 metres of coverage per box" (IFCTEXT)
    Form = "n/a" (IFCTEXT)
    Pitch = "Suitable for all pitches" (IFCTEXT)
    RollLengths = "2 x 6 metre roll lengths" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_ReconstitutedSlatesRoofSlopeVentilationFittings_450mmRafterRollVentilator" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/zuna3rjz" (IFCTEXT)
    NBSDescription = "Reconstituted slates roof slope ventilation fittings" (IFCTEXT)
    NBSReference = "45-80-90/392" (IFCTEXT)
    ProductInformation = "Universal Rafter Roll Ventilator | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_35_90_93_72" (IFCTEXT)
    Uniclass2015Title = "Reconstituted slate roof slope ventilation fittings" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)