IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2021-07-21T18:39:46"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210416_1515(x64) - Exporter 19.2.30.41 - Alternate UI 19.2.30.41"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "elisabeth.kitumaini" of Organization (no name given)
  Owner history of Person "elisabeth.kitumaini" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1626889185 (2021-07-21T17:39:45Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | object type "NBS_TapcoRoofingProducts_DryFxngAbtmnts_Tapco_AbutmentVentilator:Tapco_AbutmentVentilator" | ROOFING | names: "NBS_TapcoRoofingProducts_DryFxngAbtmnts_Tapco_AbutmentVentilator:Tapco_AbutmentVentilator:3562" | material: "NBS_TapcoRoofingProducts_Acrylonitrilebutadienestyrene(ABS)_Black" | property sets: BOS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie

Property sets
  BOS_General | properties | on 1 object (1 IFCCOVERING)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_TapcoRoofingProducts_DryFixingAbutments_Tapco_AbutmentVentilator" (IFCTEXT)
    ManufacturerName = "Tapco Roofing Products" (IFCTEXT)
    ManufacturerURL = "www.tapcoroofingproducts.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/54sxteod" (IFCTEXT)
    NBSDescription = "Dry fixing abutments" (IFCTEXT)
    NBSReference = "45-80-90/372" (IFCTEXT)
    ProductInformation = "Tapco Abutment Ventilator | Tapco Roofing Products" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_35_90_93_27" (IFCTEXT)
    Uniclass2015Title = "Dry fixing abutments" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    Accessories = "n/a" (IFCTEXT)
    Applications = "Suitable and recommended for all Tapco Roofing products, can be used in conjunction with traditional ‘lead roll’ details on slate and shake roofs, particularly suitable for Tapco Slate Classic tiles" (IFCTEXT)
    Form = "n/a" (IFCTEXT)
    Pitch = "Suitable for pitches of 20° and above" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "Polymeric resin" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  IFC | properties | on 1 object (1 IFCCOVERING)
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "ROOFING" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_90_93_27:Dry fixing abutments" (IFCTEXT)
    CodePerformance = "BS 5250" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Abutment Ventilator providing unobtrusive high-level ventilation in conjunction with lead roll details on slate and shake roofs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "25+ years" (IFCTEXT)
    Features = "Guaranteed 5000 mm²/m ventilation provision to comply with BS 5250 and Building Regulations, deluge and driving rain resistant as well as preventing large insect ingress, unobtrusive when installed. Hidden within the roof flashings, can be used with AluFlash, the lead-free alternative, each unit overlaps the next to ensure integrity of flashing, quick and easy to install. Does not affect the normal laying of the roof covering" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "international@tapcoint.com" (IFCTEXT)
    Material = "Acrylonitrile butadiene styrene (ABS)" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Tapco_AbutmentVentilator" (IFCTEXT)
    Name = "DryFixingAbutments_Tapco_AbutmentVentilator_TapcoRoofingProducts" (IFCTEXT)
    NominalHeight = 24.00000003648 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1035.0000015732 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 203.00000030856 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "1035 x 203 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "40-years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 1" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)